Walker Reserve

Topsoil should be stripped to a depth of 6 inches and all stock piles should have side slopes no steeper than 3:1 and seeded. All disturbed areas should be seeded and mulched with weed free hay mulch at 4,000 lbs. /acre. All disturbed areas should be reseeded between the planting dates of Nov. 1-April 30th. Grass seed should be drilled at a depth of ¼ to ½ inch deep and if broadcasted, double the rate. Please reseed with native grasses and see the attached native grass seed mix for your site.

Noxious weeds need to be managed and controlled prior to going to seed either by chemical, mechanical, or biological control. Please contact the El Paso County Conservation District for fact sheets on specific weed control measures for each noxious weed present on the site.

Kenneth Barker

EPCCD Board President

Kenneth Barker