EA File No. 26 - 107
Engineering Meeting Notes

	EA Meeting Date/Time:
	Tuesday, 9/29/2026 11:00 

	Parcel Number: 
	7114100017, 7114100022

	Address./Plat No./Acre:
	NW Corner CO-105 & Knollwood Drive/18110 Knollwood Dr

	Project Manager/Phone:
	Jen Uhler (719) 520-7952
	Development Services Engineer/Phone:
	Charlene Durham, PE (719) 520-7951
	Stormwater Engineer/Phone
	Zachary Jannusch (719) 500-3170
	Application/Land Use Type:        

	Rezone & Final Plat



IMPORTANT NOTE:
These Engineering meeting notes are based on the information provided by the Applicant and reasonable preliminary research.  The County requirements and policies in effect at the time of the meeting may change prior to the project submittal date, and the requirements and policies in effect at the date of submittal shall apply.  Based on the applicant-provided information and preliminary research, these notes are the best estimate of the requirements expected to be met by the Applicant.  The actual requirements may change based on project revisions, new information, or constraints that were unavailable or overlooked at the time of the Early Assistance meeting.  It is solely the Applicant’s responsibility to research and be familiar with state and federal laws and permitting requirements; the County’s regulations, codes and criteria; the requirements of other applicable local, state or federal agencies; and any governing documents that apply to the project, including previous drainage and transportation studies and previous land use approvals and conditions. Reference links are provided at the end of this document. 
REQUEST
	Rezone of approximately 1.70 AC (74,185 SF) from Rural Residential (RR-5) to Commercial Community (CC) and a subsequent subdivision of the applicable properties.




Drainage Impacts
Requirements
	Documents
	Design Elements

	☐	Drainage Basin Planning Study (DBPS)
	☒	Full Spectrum Detention 

	☐	Master Development Drainage Plan (MDDP)
	☒	Permanent Water Quality 

	☒	Preliminary/Final Drainage Report/Letter Final Plat and SDP
	☒	Downstream Conveyance Analysis (to include possible offsite improvements)

	☒	Financial Assurance Estimate (FAE) Form SDP only
	☒	Floodplain Impacts

	☐	Builder’s Erosion and Stormwater Quality Control Permit (BESQCP)
	☐	Public Improvements

	☒	Erosion and Stormwater Quality Control Permit (ESQCP) SDP only
	
	

	☒	Grading & Erosion Control (GEC) Plan & GEC Checklist SDP only
	Miscellaneous

	☒	Stormwater Management Plan (SWMP) & SWMP Checklist SDP only
	☐	Construction Activity Permit/ CDPHE Discharge Permit/CDPHE APEN Fee

	☒	PCM Applicability Form SDP only
	☐	Special Districts/Water Quality Authority Areas

	☐	PCM Maintenance Agreement and O&M Manual
	
	

	☒	MHFD-Detention Basin Design Workbook or SDI Sheet SDP only
	
	

	☐	Pre-Subdivision Site Grading Form
	
	

	☐	Deviation Request
	
	



	Basin Name/Studied
	Basin Fee1, 2
	Bridge Fee1

	Dirty Woman Creek Drainage Basin
	$27,282
	$1492

	
	
	

	
	
	


1 Per impervious acre, collected prior to recordation of Final Plat. Fee amounts are based on the current fee schedule at the time of the Early Assistance meeting. Fees are subject to change. 
2 A 25% fee reduction applies for low density residential lots (2.5 acres and greater lot sizes). The reduction only applies to the basin fee. 

Drainage Notes: 
· Rezone does not require drainage documents. 
· A Drainage report completed by a professional engineer licensed in the state of Colorado will be required with Final Plat application. As the actual commercial project is not yet known, provide a drainage memo discussing highest and best use for the site and how that works with the assumed design of the existing pond to the west. Note that final design will done with the site plan. Items under Design Elements, will just need to be discussed within report.
· A Geotech report will be required to meet CGS and County standards and is submitted with the Final Plat application. 
· Drainage basin & bridge fees are applicable at Final Plat application. 
· Portion of Site is located within FEMA floodplain. Floodplain should be located within a no build/drainage easement.
· Disturbance >1ac or 500cy requires Stormwater permit. 
· An EPC Stormwater Permit (ESQCP) will be needed if/when one of the following criteria are triggered:
· Develop the site and disturb >1ac of soil, or:
· <1ac of soil disturbance but the site is part of a larger common plan of development, or: 
· Cut and/or fill >500 cubic yards of soil, or:
· The site is located in or adjacent to a sensitive area.
· If/when the site disturbs >1ac of soil, a stormwater quality treatment facility (PCM) will be needed for the runoff from the non-excluded areas. Exclusions can be found in our PCM Applicability Form and ECM Appendix I.6.1.B
· EPC Hwy 105 Pond accounted for development of this area, see excerpt below
· The pond’s orifice plate will need to be redesigned and replaced to meet drain time criteria
· Pond will be maintained by EPC
From Highway 105 Project A FDR:
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[image: ]
Traffic Impacts
Requirements
	☒	Traffic Impact Study/Memorandum 
	☒
	Road Impact Fee – Due at Building Permit                                      
	☐
	Joint Access Easement

	☐	Road Construction Plans
	☒	Road Impact Fee Acknowledgement Form                        
	☐	County/CDOT project coordination required

	☐	Public Improvements
	☒	Driveway Access Permit                        
	☐	Outsourcing of Traffic Impact Study

	☐	Deviation Request
	☐	Signal Warrant Study
	☐	New Road Access Permit



	Adjacent Road Name
	Ex. ROW (ft)
	Surface 
	PCI Rating
	2045 MTCP
	2065 MTCP
	Required Intersection Spacing (ft)

	
	
	
	
	Classification
	ROW
	Dedication
	Classification
	ROW
	Potential Preservation 
	

	Knollwood Blvd – West of Knollwood Dr
	Private
	Gravel
	N/A
	
	
	
	
	
	
	

	Knollwood Blvd – East of Knollwood Dr
	60 – Rural Local
	Asphalt
	91
	
	
	
	
	
	
	

	Knollwood Dr
	60-Rural Local
	Asphalt
	70
	
	
	
	
	
	
	

	Highway 105
	100 – Urb Prin Art
	Asphalt
	70
	
	
	
	
	
	
	

	Village Ridge Pt
	Private
	Unimp
	N/A
	
	
	
	
	
	
	

	
	Other (i.e. multi-jurisdictional):

	Metro District
	
	Choose an item.



Traffic Notes:
· A Traffic Impact Study is required unless all criteria are satisfied in ECM B.1.2.D. 
· TIS should address fullest and best use of the lot and development. Intersections and access points below to be analyzed and included in the TIS. 
· El Paso County Road Impact Fee program is applicable to this development. Fees are due at the time of building permit approval. 
· https://publicworks.elpasoco.com/road-impact-fees/
· A Driveway Access Permit is required before any access is established from the proposed lots to the proposed roadway. The application can be completed online via EDARP: https://epcdevplanreview.com/Applications/Create_Email 


Anticipated Engineering Review and Construction Permit Fees

	Engineering Application 
	Review Fee1

	
	

	
	

	
	

	
	



1 Fee amounts are based on the current fee schedule at the time of the Early Assistance meeting. Fees are subject to change. 

Full Fee Schedule: https://planningdevelopment.elpasoco.com/#1515613078895-69552b09-44a4



COUNTY CODES AND CRITERIA:
El Paso County Land Development Code (LDC) (2016): https://planningdevelopment.elpasoco.com/land-development-code/
El Paso County Engineering and Drainage Criteria Manuals (ECM) (2020) & (DCM) Volumes 1 and 2 and Update: 
https://planningdevelopment.elpasoco.com/planning-community-development/engineering/#1519834440345-f2ddfd20-0d90
El Paso County 2045 Major Transportation Corridors Plan (MTCP) Update: https://publicworks.elpasoco.com/department-public-works/major-transportation-corridors-2045-update/ 
El Paso County Road Impact Fee Program: https://publicworks.elpasoco.com/road-impact-fees/ 
El Paso County Development Fees: https://planningdevelopment.elpasoco.com/#1515613078895-69552b09-44a4
El Paso County Projects (EDARP):  https://epcdevplanreview.com/Public 
El Paso County Municode Library: https://library.municode.com/co/el_paso_county
Planning and Community Development: https://planningdevelopment.elpasoco.com/planning-development-forms/#1643393391537-a0dac52d-1b3b 
El Paso County Stormwater Page: https://publicworks.elpasoco.com/stormwater/ 
Assessor’s Information 
Assessor’s Data:  https://property.spatialest.com/co/elpaso/#/  		Assessor’s Map:  https://community.spatialest.com/co/elpaso/#/Property-Search/ 
Drainage Links:
Mile High Flood District: http://MHFD.org 
Detention Pond Compliance Website: https://maperture.digitaldataservices.com/gvh/?viewer=cswdif 
State DWR: http://water.state.co.us/SURFACEWATER/DAMSAFETY/Pages/DamSafety.aspx 
NOAA Rainfall: https://hdsc.nws.noaa.gov/hdsc/pfds/pfds_map_cont.html?bkmrk=co 
Floodplain: https://www.pprbd.org/Download/Floodplain#floodplainHandouts
https://pprbd.maps.arcgis.com/apps/webappviewer/index.html?id=1d9243f3606542159a0a418070b08686
https://msc.fema.gov/portal/advanceSearch
Fountain Creek Watershed: http://www.fountain-crk.org/ 
Upper Black Squirrel Creek Ground Water Management District Mapping Study: https://upperblacksquirrelcreekwater.com/waterStudies.php 
Water Rights:
Colorado Division of Natural Resources: https://dwr.state.co.us/Portal/dwr/AskDWR
State Transportation Links
Colorado Department of Transportation (CDOT) M&S Standards and Specifications, Access Code and Permit:
· https://www.codot.gov/business/designsupport/standard-plans 
· https://www.codot.gov/business/permits/accesspermits
· https://www.codot.gov/business/permits/accesspermits/references

Local Governing Authorities
City of Colorado Springs: https://coloradosprings.gov/ 	
City of Fountain: https://www.fountaincolorado.org/ 			
Town of Calhan: http://calhan.co/ 			
Green Mountain Falls: https://gmfco.elpasoco.com/ 
Town of Monument: http://www.townofmonument.org/ 			
Town of Palmer Lake: http://www.townofpalmerlake.com/ 
Contact Information 
	CDOT R2 Permits Program Manager 
	(719)562-5540

	Work in Right of Way Permit 
	(719)520-6869

	Right of Way Vacation 
	(719)520-6897

	Floodplain Administrator 
	(719)327-2898

	EPC Public Health 
	(719)578-3199

	CDPHE Air Quality Division 
	(303)692-3100

	CDPHE Water Quality Division 
	(303)692-3500

	Cherry Creek Basin Water Quality Authority 
	(303)239-5400





Traffic Information 
	Traffic Impact Study (ECM Appendix B)*

	Full TIS
	ADT > 1,000 or Pk Hr > 100

	Intermediate TIS
	ADT < 1,000 or Pk Hr < 100

	Traffic Memo
	ADT ≤ 500    or Pk Hr ≤ 50

	No TIS
	ADT < 100    or Pk Hr < 10


*An approved TIS that has been prepared in the last three years may be revised or updated where a proposed access is changed or a change in the proposed action may result in a new trip generation that exceeds the original trip generation estimates. An amendment letter is required. 
**If the original TIS is older than three years, an entirely new TIS shall be prepared. 
***Any submitted TIS is subject to third party review based on size and complexity, in which additional fees will be assessed to the applicant. 
The applicant is responsible for obtaining any necessary approvals for impacts within other jurisdictions. It is recommended that the applicant approach the jurisdiction early in the development process for any additional requirements. If the proposal is impacted by an El Paso County Department of Public Works project, coordination with DPW is required. 
Pavement Condition Index
The Pavement Condition Index (PCI) is a numerical rating system that measures the condition of a road's pavement on a scale of 0 to 100. A score of 100 indicates a newly paved road, while 0 is the worst possible condition. The PCI is calculated based on the type and severity of distresses observed on the pavement surface, such as cracking, rutting, scaling, and spalling. Other factors that can affect the PCI score include Pavement age, Climate and precipitation, Traffic loads, and maintenance. 
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Drainage Report/Plan Information 
	Drainage Basin Planning Study (DBPS) – May be required with a very large development

	Master Development Drainage Plan (MDDP) – Required with phased development greater than 10 acres (may be required with Sketch Plan) (DCM Section 4.2)

	Drainage Letter Report – With a Re-plat, Minor Sub or Plot Plan (DCM Section 4.5) where a final drainage report has previously been approved.

	Preliminary Drainage Report (PDR) – Required with a Preliminary Plan (DCM Section 4.3)

	Final Drainage Report (FDR) – Required with a Final Plat (DCM Section 4.4)


Drainage Master Plan/Floodplain Information 
If it is undetermined at this time if an adopted Drainage Basin Planning Study (DBPS) or Master Plan exists in this area, the applicant is responsible for researching the appropriate information.
If the subdivision application impacts the FEMA floodplain, a FEMA Letter of Map Revision may be required. If the site is in or near a floodplain, contact the Regional Floodplain Administrator for allowed floodplain uses and procedural requirements. It is the Applicant’s responsibility to research the effects and implications of developing in or near a floodplain, including limited uses, floodplain development permits, geotechnical, wetland and wildlife studies, structural requirements, flood insurance and potential future floodplain mapping updates. FEMA's FIRM maps may be out of date or at a low level of accuracy.
If the site lies within the Cherry Creek Basin Water Quality Authority area and is not rural density, the applicant should discuss any concerns related to the development with the CCBWQA’s consultant. 
If the site lies within the Fountain Creek watershed, the District has authority over the floodplain impacts and is advisory to the County on uses outside of the floodplain. The applicant should discuss any concerns related to the development with District staff. 
Detention/Water Quality PCM & Downstream Conveyance Information 
Per ECM Chapter 3.2.8.B: “The proposed project or developed land use shall not change historical runoff values, cause downstream damage, or adversely impact adjacent properties.” 
The project must provide an acceptable method of storm drainage conveyance and may be required to construct (or contribute an equitable share to the construction of) a storm conveyance or collector system. 
If the site conveys storm drainage flows through or across an adjacent private property, then the applicant is responsible for obtaining off-site drainage easements in accordance with the Engineering Criteria Manual Section 3.3.3.K. Any offsite easements necessary for the development shall be recorded prior to County Plan approvals. 
If on-site facilities are required, the applicant will be required to provide access and drainage easements in accordance with Section 11.2.2 of the Drainage Criteria Manual.
If a water quality and/or detention facility is applicable, some or all of the following documents may be required: Operation and Maintenance (O&M) Manual, Private Detention Basin / Stormwater Quality BMP (ie: PCM) Maintenance Agreement, and Stormwater Detention and Infiltration (SDI) Form.
For post-construction water quality PCM requirements, see Appendix I of the Engineering Criteria Manual. If/when the site disturbs >1ac of non-excluded areas, a stormwater quality treatment facility (ie: PCM) will be needed for the runoff from the non-excluded areas. Exclusions can be found in our PCM Applicability Form and ECM Appendix I.7.1.
State Engineer’s requirements regarding dams and water rights apply. Jurisdictional/Non-Jurisdictional dam construction forms are typically required for detention facilities. If applicable, provide proof of submittal of the State’s “Notice of Intent to Construct a Non-Jurisdictional Water Impoundment Structure” form. 


Grading, Erosion, and Sediment Control Information
The Grading and Erosion Control (GEC) Plan must be prepared in accordance with Drainage Criteria Manual Vol. 2, Chapter 3 and the County’s GEC Checklist. 
An Erosion and Stormwater Quality Control Permit (ESQCP) and Permanent Control Measure are required for the following conditions per ECM Appendix I.4:
· Construction activities that result in land disturbance of greater than or equal (≥) to one acre, or
· Construction activities that result in less than (<) one acre if the activity is part of a larger “Common Plan of Development or Sale” (ECM Chapter 1.22) that would disturb one acre or more of ground surface
An ESQCP may be required as determined by the ECM Administrator for the following conditions per ECM Appendix I.4:
· Construction activities that are located in or adjacent to a Sensitive Area, or
· Cut and/or fill greater than (>) 500 cubic yards of soil
See the three ESQCP exclusions listed in ECM Chapter 5.6.3.
An application for an ESQCP shall be accompanied by the following: 
	· Drainage Report
· ESQCP Form
· Financial Surety 
· GEC Plan and GEC Checklist

	· PCM Applicability Form
· Stormwater Management Plan (SWMP) and SWMP Checklist
· O&M Manual (for sites requiring a PCM)
· PCM Maintenance Agreement (for sites requiring a PCM


A Builder’s Erosion and Stormwater Quality Control Permit (BESQCP) is required for residential building lots with < 1 acre of disturbed areas and does not meet any of the criteria for an ESQCP listed above. 
Construction activities that disturb >1ac of soil are required by the Environmental Protection Agency (EPA) to obtain a Construction Stormwater Permit through the Colorado Department of Public Health & Environment (CDPHE) Water Quality Control Divisions. For projects with soil disturbances >1ac but <25ac, a County Construction Activity Permit is required, contact El Paso County’s Public Health Department for further information regarding the permit. All land development activities greater than twenty-five (25) acres or with construction duration longer than six (6) months must obtain an Air Pollution Emission Notice and Emissions Permit through CDPHE’s Air Quality Control Division. 
Deviations 
All engineering designs and studies shall be performed in conformance with adopted codes, standards and criteria. Any deviations are to be formally identified and requested in writing, with justification provided per ECM Section 5.8. All deviation requests must be approved by the ECM Administrator prior to submitting the application for review, or delays in the review and additional fees may result. The Applicant must submit adequate justification for consideration of the request(s).
Public Improvements Information
If public improvements are required, the applicant will be required to enter into a Subdivision Improvement Agreement (SIA) or a development agreement (if the project is not a subdivision) with the County. Refer to the El Paso County Land Development Code for information on the SIA and the ECM for the required format of the associated Financial Assurance Estimate. All forms are available online. 
Construction drawings for the required public improvements must be reviewed and approved by PCD and the County Engineer. All Construction drawing submittals shall adhere to the criteria set forth in the ECM. A construction plan review fee will be assessed when the plans are submitted for review.    
Geotechnical reports for earthwork and pavement designs must be reviewed and approved.  All submittals must adhere to the criteria set forth in the ECM.  
Any work within the Right of Way will require a permit from El Paso County Department of Public Works. 
Any Fire cistern(s) and mailbox kiosks need to be shown on the construction drawings. 
Metro District Fees
	Woodmen Road Metro District
	Central Marksheffel Metro District
	Lorson Ranch Metro District
	Constitution Heights Metro District

	· Effective January 1, 2026, El Paso County collects and keeps fees set by district.
· After December 31, 2020 no property in the Amended Service Area shall be permitted to join the WRMD, and shall participate fully in the Fee Program.
· As of January 1, 2021 and until either bonds retire or December 31, 2027, whichever occurs sooner, El Paso County must pay a portion of the Road Impact Fee it collects from property in the Amended Service Area that receives final plat approval to WRMD.
	· Property in district pays no fee
· District granted $2.9 million in Fee Program Credit 
· Fee Program will pay annual credit reimbursements to District, or can sell credits 
	· Property in district pays full fee
· District granted $4.1 million in credit 
· Credits used toward future development, can apply for reimbursement, can sell credits
	· Property in district pays full fee
· District granted $3.1 million in credit 
· Used toward future development, can sell credits, NO reimbursement
· County will collect building permit fees for reimbursement of PPRTA improvements to Marksheffel Road from property within District and some property outside District – Credit given toward Impact Fee for amount of building permit fee paid. 


*Properties within the Meridian Crossing subdivision are not subject to the county wide road impact fee. 
Page 1 of 11
image3.png
Pavement Condition Index

86-100
71-85
56-70
4155
26-40
11-25
0-10





image4.png
Pavement Condition Index (PCI)

100

®
S

@
S

40

20

Good L\_

Fair | nentatsreszsun |

Poor

RN L I A (A

I
A
Pavement Age

L s |




image1.png
In addition, the pond is designed with capacity to provide up to an additional 0.034 WQCV and
0.225 acre-feet of volume for an anticipated future development that may be constructed at the
corner of Hwy 105 and Knollwood Dr. Anticipated areas are as per conversations with the
property owner’s representative and allow for conversion of 0.8 acres of undeveloped area to
impervious area along with additional tributary area of 0.5 acres. Areas are reflected in the
Rational Method Calculations in Appendix D. Calculations for the pond design are reflected in
Appendix F. This includes the spreadsheet for the pond design and outlet structure design for
the roadway project (interim condition) and the spreadsheet for the pond design with the
proposed development (final condition). The pond was designed per El Paso County criteria as
of February 9, 2023.
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